Martin Villasenor

CC1350 TI-RTOS/RF LAB2

**11/16/2018**

**------------------------------------------------------------------------------------**

Youtube Link: <https://youtu.be/2mnE_Pd4j98>

**Modified Code:**

/\*

\* ======== empty.c ========

\*/

/\* For usleep() \*/

**#include** <unistd.h>

**#include** <stdint.h>

**#include** <stddef.h>

/\* Driver Header files \*/

**#include** <ti/drivers/GPIO.h>

**#include** <ti/drivers/ADC.h>

**#include** <ti/display/Display.h>

// #include <ti/drivers/I2C.h>

// #include <ti/drivers/SDSPI.h>

// #include <ti/drivers/SPI.h>

// #include <ti/drivers/UART.h>

// #include <ti/drivers/Watchdog.h>

/\* Board Header file \*/

**#include** "Board.h"

// Global variables for GUI COMPOSER

uint16\_t adcValue = 0;

uint16\_t threshold = 100;

uint16\_t trigger = 0;

/\*

\* ======== gpioButtonFxn0 ========

\* Callback function for the GPIO interrupt on Board\_GPIO\_BUTTON0.

\*/

**void** **gpioButtonFxn0**(uint\_least8\_t index)

{

/\* Clear the GPIO interrupt and decrement threshold \*/

**if**(threshold < 250){ // Ensure threshold doesn't go below zero

threshold = 0;

} **else** {

threshold -= 250; // decrement by 250

}

}

/\*

\* ======== gpioButtonFxn1 ========

\* Callback function for the GPIO interrupt on Board\_GPIO\_BUTTON1.

\* This may not be used for all boards.

\*/

**void** **gpioButtonFxn1**(uint\_least8\_t index)

{

/\* Clear the GPIO interrupt and increment threshold \*/

**if**(threshold > 16133){ // Ensure threshold doesn't go above max ADC range

threshold = 16383;

} **else** {

threshold += 250; // increment by 250

}

}

/\*

\* ======== mainThread ========

\*/

**void** \***mainThread**(**void** \*arg0)

{

/\* 1 second delay

uint32\_t time = 1;

\*/

// ~10 loops/second

uint32\_t time = 100000;

/\* Call driver init functions \*/

**GPIO\_init**();

**ADC\_init**();

// I2C\_init();

// SDSPI\_init();

// SPI\_init();

// UART\_init();

// Watchdog\_init();

//Open Display Driver

Display\_Handle displayHandle;

Display\_Params displayParams;

Display\_Params\_init(&displayParams);

displayHandle = Display\_open(Display\_Type\_UART, NULL);

// Open ADC Driver

ADC\_Handle adc;

ADC\_Params params;

**ADC\_Params\_init**(&params);

adc = **ADC\_open**(Board\_ADC0, &params);

**if**(adc == NULL){

// Error initializing ADC Channel 0

**while** (1);

}

/\* install Button callback \*/

**GPIO\_setCallback**(Board\_GPIO\_BUTTON0, gpioButtonFxn0);

**GPIO\_setCallback**(Board\_GPIO\_BUTTON1, gpioButtonFxn1);

/\* Enable interrupts \*/

**GPIO\_enableInt**(Board\_GPIO\_BUTTON0);

**GPIO\_enableInt**(Board\_GPIO\_BUTTON1);

**while**(1){

int\_fast16\_t res;

res = **ADC\_convert**(adc, &adcValue);

**if** (res == ADC\_STATUS\_SUCCESS) {

Display\_printf(displayHandle, 1,0, "ADC Reading %d", adcValue);

**if** (adcValue >= threshold){

**GPIO\_write**(Board\_GPIO\_LED0, Board\_GPIO\_LED\_ON);

trigger = 1;

} **else**{

**GPIO\_write**(Board\_GPIO\_LED0, Board\_GPIO\_LED\_OFF);

trigger = 0;

}

}

**usleep**(time);


}

}


**Code was modified to add global variables for the adc value, threshold and LED reading.**

**After creating project, via XDS110 interface flashed the empty\_CC1350\_LAUNCHXL\_tirtos\_ccs.out CC1350 board. Once connected**


**An application was created on http://dev.ti.com/gc**




Gauge properties



**Slider properties**



**LED properties**



**Application running on separate page. Showing gauge, slider and LED indicators.**

